# DE-Nano FPGA Board Configuration

## Pin Assignments:

- CLOCK
- LED
- KEY
- SW
- SDRAM
- Accelerometer and EEPROM
- GPIO_0
- GPIO_0

## Pin Assignment Table:

##

CLOCK
Name | Location | Direction | Standard
--- | --- | --- | ---
CLOCK_50 | R8 | input | 3.3-V LVTTL

##

LED
Name | Location | Direction | Standard
--- | --- | --- | ---
LED[0] | A15 | output | 3.3-V LVTTL
LED[1] | A13 | output | 3.3-V LVTTL
LED[2] | B13 | output | 3.3-V LVTTL
LED[3] | A11 | output | 3.3-V LVTTL
LED[4] | D1 | output | 3.3-V LVTTL
LED[5] | F3 | output | 3.3-V LVTTL
LED[6] | B1 | output | 3.3-V LVTTL
LED[7] | L3 | output | 3.3-V LVTTL

##

KEY
Name | Location | Direction | Standard
--- | --- | --- | ---
KEY[0] | J15 | input | 3.3-V LVTTL
KEY[1] | E1 | input | 3.3-V LVTTL

##

SW
Name | Location | Direction | Standard
--- | --- | --- | ---
SW[0] | M1 | input | 3.3-V LVTTL
SW[1] | T8 | input | 3.3-V LVTTL
SW[2] | B9 | input | 3.3-V LVTTL
SW[3] | M15 | input | 3.3-V LVTTL

##

SDRAM
Name | Location | Direction | Standard
--- | --- | --- | ---
DRAM_BA[0] | M7 | output | 3.3-V LVTTL
DRAM_BA[1] | M6 | output | 3.3-V LVTTL
DRAM_DQM[0] | R6 | output | 3.3-V LVTTL
DRAM_DQM[1] | T5 | output | 3.3-V LVTTL
DRAM_RAS_N | L2 | output | 3.3-V LVTTL
DRAM_CAS_N | L1 | output | 3.3-V LVTTL
DRAM_CKE | L7 | output | 3.3-V LVTTL
DRAM_CLK | R4 | output | 3.3-V LVTTL
DRAM_WE_N | C2 | output | 3.3-V LVTTL
DRAM_CS_N | P6 | output | 3.3-V LVTTL
DRAM_DQ[0] | G2 | inout | 3.3-V LVTTL
DRAM_DQ[1] | G1 | inout | 3.3-V LVTTL
DRAM_DQ[2] | L8 | inout | 3.3-V LVTTL
DRAM_DQ[3] | K5 | inout | 3.3-V LVTTL
DRAM_DQ[4] | K2 | inout | 3.3-V LVTTL
DRAM_DQ[5] | J2 | inout | 3.3-V LVTTL
DRAM_DQ[6] | J1 | inout | 3.3-V LVTTL
DRAM_DQ[7] | R7 | inout | 3.3-V LVTTL
DRAM_DQ[8] | T4 | inout | 3.3-V LVTTL
DRAM_DQ[9] | T2 | inout | 3.3-V LVTTL
DRAM_DQ[10] | T3 | inout | 3.3-V LVTTL
DRAM_DQ[11] | R3 | inout | 3.3-V LVTTL
DRAM_DQ[12] | R5 | inout | 3.3-V LVTTL
DRAM_DQ[13] | P3 | inout | 3.3-V LVTTL
DRAM_DQ[14] | N3 | inout | 3.3-V LVTTL
DRAM_DQ[15] | K1 | inout | 3.3-V LVTTL
DRAM_ADDR[0] | P2 | output | 3.3-V LVTTL
DRAM_ADDR[1] | N5 | output | 3.3-V LVTTL
DRAM_ADDR[2] | N6 | output | 3.3-V LVTTL
DRAM_ADDR[3] | M8 | output | 3.3-V LVTTL
DRAM_ADDR[4] | P8 | output | 3.3-V LVTTL
DRAM_ADDR[5] | T7 | output | 3.3-V LVTTL
DRAM_ADDR[6] | N8 | output | 3.3-V LVTTL
DRAM_ADDR[7] | T6 | output | 3.3-V LVTTL
DRAM_ADDR[8] | R1 | output | 3.3-V LVTTL
DRAM_ADDR[9] | P1 | output | 3.3-V LVTTL
DRAM_ADDR[10] | N2 | output | 3.3-V LVTTL
DRAM_ADDR[11] | N1 | output | 3.3-V LVTTL
DRAM_ADDR[12] | L4 | output | 3.3-V LVTTL

##

Accelerometer and EEPROM
Name | Location | Direction | Standard
--- | --- | --- | ---
I2C_SCLK | F2 | output | 3.3-V LVTTL
I2C_SDAT | F1 | inout | 3.3-V LVTTL
G_SENSOR_CS_N | G5 | output | 3.3-V LVTTL
G_SENSOR_INT | M2 | input | 3.3-V LVTTL

##

GPIO_0 connect to LTM - 4.3" LCD and Touch
Name | Location | Direction | Standard | GPIO Pin Index
--- | --- | --- | --- | ---
LTM_ADC_PENIRQ_n | A8 | input | 3.3-V LVTTL | 1
LTM_ADC_DOUT | D3 | input | 3.3-V LVTTL | 2
LTM_ADC_BUSY | B8 | input | 3.3-V LVTTL | 3
LTM_ADC_DIN | C3 | output | 3.3-V LVTTL | 4
LTM_ADC_DCLK | A2 | output | 3.3-V LVTTL | 5
LTM_B[3] | A3 | output | 3.3-V LVTTL | 6
LTM_B[2] | B3 | output | 3.3-V LVTTL | 7
LTM_B[1] | B4 | output | 3.3-V LVTTL | 8
LTM_B[0] | A4 | output | 3.3-V LVTTL | 9
LTM_NCLK | B5 | output | 3.3-V LVTTL | 10
LTM_DEN | A5 | output | 3.3-V LVTTL | 13
LTM_HD | D5 | output | 3.3-V LVTTL | 14
LTM_VD | B6 | output | 3.3-V LVTTL | 15
LTM_B[4] | A6 | output | 3.3-V LVTTL | 16
LTM_B[5] | B7 | output | 3.3-V LVTTL | 17
LTM_B[6] | D6 | output | 3.3-V LVTTL | 18
LTM_B[7] | A7 | output | 3.3-V LVTTL | 19
LTM_G[0] | C6 | output | 3.3-V LVTTL | 20
LTM_G[1] | C8 | output | 3.3-V LVTTL | 21
LTM_G[2] | E6 | output | 3.3-V LVTTL | 22
LTM_G[3] | E7 | output | 3.3-V LVTTL | 23
LTM_G[4] | D8 | output | 3.3-V LVTTL | 24
LTM_G[5] | E8 | output | 3.3-V LVTTL | 25
LTM_G[6] | F8 | output | 3.3-V LVTTL | 26
LTM_G[7] | F9 | output | 3.3-V LVTTL | 27
LTM_R[0] | E9 | output | 3.3-V LVTTL | 28
LTM_R[1] | C9 | output | 3.3-V LVTTL | 31
LTM_R[2] | D9 | output | 3.3-V LVTTL | 32
LTM_R[3] | E11 | output | 3.3-V LVTTL | 33
LTM_R[4] | E10 | output | 3.3-V LVTTL | 34
LTM_R[5] | C11 | output | 3.3-V LVTTL | 35
LTM_R[6] | B11 | output | 3.3-V LVTTL | 36
LTM_R[7] | A12 | output | 3.3-V LVTTL | 37
LTM_GREST | D11 | output | 3.3-V LVTTL | 38
LTM_SCEN | D12 | output | 3.3-V LVTTL | 39
LTM_SDA | B12 | inout | 3.3-V LVTTL | 40

##

GPIO_1 connect to D5M - 5M Pixel Camera
Name | Location | Direction | Standard | GPIO Pin Index
--- | --- | --- | --- | ---
D5M_PIXCLK | T9 | input | 3.3-V LVTTL | 1
D5M_D[11] | F13 | input | 3.3-V LVTTL | 2
D5M_D[10] | T15 | input | 3.3-V LVTTL | 4
D5M_D[9] | T14 | input | 3.3-V LVTTL | 5
D5M_D[8] | T13 | input | 3.3-V LVTTL | 6
D5M_D[7] | R13 | input | 3.3-V LVTTL | 7
D5M_D[6] | T12 | input | 3.3-V LVTTL | 8
D5M_D[5] | R12 | input | 3.3-V LVTTL | 9
D5M_D[4] | T11 | input | 3.3-V LVTTL | 10
D5M_D[3] | T10 | input | 3.3-V LVTTL | 13
D5M_D[2] | R11 | input | 3.3-V LVTTL | 14
D5M_D[1] | P11 | input | 3.3-V LVTTL | 15
D5M_D[0] | R10 | input | 3.3-V LVTTL | 16
D5M_XCLKIN | N9 | output | 3.3-V LVTTL | 19
D5M_RESET_N | N11 | output | 3.3-V LVTTL | 20
D5M_TRIGGER | K16 | output | 3.3-V LVTTL | 22
D5M_STROBE | R16 | input | 3.3-V LVTTL | 23
D5M_LVAL | L15 | input | 3.3-V LVTTL | 24
D5M_FVAL | P15 | input | 3.3-V LVTTL | 25
D5M_SDATA | P16 | inout | 3.3-V LVTTL | 26
D5M_SCLK | R14 | output | 3.3-V LVTTL | 27